<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<hole x="48.26" y="71.12" drill="2"/>
<hole x="85.09" y="71.12" drill="2"/>
<hole x="85.09" y="24.13" drill="2"/>
<hole x="48.26" y="24.13" drill="2"/>
<text>+
3-5
V
_</text>
<text>ATtiny
25/45/85[V]

ATmega 
8/168/328[V]</text>
<text>se-it.eu</text>
</plain>
<libraries>
<library name="con-ml">
<packages>
<package name="ML6">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="E2,5-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 5 mm</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CERM_OSC">
</package>
<package name="DO-1N4148">
</package>
</packages>
</library>
<library name="con-wago-500">
<description>&lt;b&gt;Wago Screw Clamps&lt;/b&gt;&lt;p&gt;
Grid 5.00 mm&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="W237-102">
<description>&lt;b&gt;WAGO SCREW CLAMP&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="avr-7">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Version 7 - August 1, 2011.&lt;br&gt;&lt;br&gt;
Added ATmega164P/324P/644P devices for DIP and TQFP.
&lt;p&gt;
Version 4 - March 11, 2008.&lt;br&gt;&lt;br&gt;
This library now includes ONLY ATMEL AVR microcontrollers.  It is the result of merging all other available device libraries available at http://www.cadsoft.de/download as of the time it was made.  In addition to the legacy AT90* devices, it includes most ATMEGA devices including the new 48/88/168, most ATTiny devices and a set of ISP and JTAG pin headers.&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt; file at90smcu_v400.zip
&lt;li&gt;avr.lbr and atmel.lbr as provided by CadSoft
&lt;li&gt;avr-1.lbr by David Blundell
&lt;li&gt;avr-2.lbr by Boris Zalokar
&lt;li&gt;avr-3.lbr by Carson Reynolds
&lt;li&gt;attiny24_44_84.lbr by Pawel Szramowski (ATTiny24/44/84 devices)
&lt;li&gt;atmel.lbr by Bob Starr (ISP headers)
&lt;li&gt;moates_custom_parts.lbr (edge ISP)
&lt;li&gt;other misc sources
&lt;/ul&gt;
&lt;author&gt;Revised by David Blundell (blundar at gmail dot com) and others.&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added Mega162, Tiny2313 John Lussmyer (cougar at casadelgato.com)&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added XMega A1,A3,A4,D3,D4 John Lussmyer Aug 1, 2011(cougar at casadelgato.com)&lt;/author&gt;</description>
<packages>
<package name="DIL28-3">
<description>&lt;B&gt;Dual In Line&lt;/B&gt; 0.3 inch</description>
</package>
</packages>
</library>
<library name="se-it.eu.eagle-library">
<packages>
<package name="1X04-BIG">
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="rcl" package="0207/10" value="10k"/>
<element name="SV1" library="con-ml" package="ML6" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="U$1" library="adafruit" package="CERM_OSC" value="4.0 MHz"/>
<element name="C1" library="rcl" package="E2,5-5" value="100uF"/>
<element name="X1" library="con-wago-500" package="W237-102" value="">
<attribute name="OC_NEWARK" value="70K9898"/>
<attribute name="MPN" value="237-102"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="IC1" library="avr-7" package="DIL28-3" value="MEGA8-P"/>
<element name="JP1" library="se-it.eu.eagle-library" package="1X04-BIG" value=""/>
<element name="JP2" library="se-it.eu.eagle-library" package="1X04-BIG" value=""/>
<element name="D1" library="adafruit" package="DO-1N4148" value="1N4148"/>
<element name="U$2" library="adafruit" package="CERM_OSC" value="8.0 MHz"/>
<element name="IC2" library="atmel" package="DIL08" value="TINY10P">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$1" pad="P$3"/>
<contactref element="JP1" pad="2"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="P$1"/>
<contactref element="JP1" pad="3"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="GND">
<contactref element="SV1" pad="6"/>
<contactref element="U$1" pad="P$2"/>
<contactref element="C1" pad="-"/>
<contactref element="X1" pad="2"/>
<contactref element="JP1" pad="4"/>
<contactref element="U$2" pad="P$2"/>
<contactref element="IC2" pad="4"/>
<contactref element="IC2" pad="4"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="VCC2">
<contactref element="R1" pad="2"/>
<contactref element="SV1" pad="2"/>
<contactref element="C1" pad="+"/>
<contactref element="JP2" pad="1"/>
<contactref element="IC2" pad="8"/>
<contactref element="IC2" pad="8"/>
<contactref element="D1" pad="C"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="1"/>
<contactref element="SV1" pad="5"/>
<contactref element="IC1" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="SV1" pad="4"/>
<contactref element="IC1" pad="17"/>
<contactref element="JP2" pad="4"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="SV1" pad="3"/>
<contactref element="IC1" pad="19"/>
<contactref element="JP2" pad="2"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="N$6">
<contactref element="SV1" pad="1"/>
<contactref element="IC1" pad="18"/>
<contactref element="JP2" pad="3"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="N$8">
<contactref element="U$2" pad="P$1"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="N$9">
<contactref element="U$2" pad="P$3"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="N$7">
<contactref element="D1" pad="A"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="N$10">
</signal>
</signals>
</board>
</drawing>
</eagle>
